|  |  |
| --- | --- |
| **Fall Winter Outside** |  |
| Drain outdoor faucets and hoses. |  |
| Clean gutters and downspouts. |  |
| Repair broken, cracked glass. |  |
| Cover window air conditioner for the Winter. |  |
| Check exhaust ducts are clear (birds or insect nests). |  |
| To prevent ice dams, use a roof rake to remove excess  snow from the edges of the roof. (Google Ice Dams to see how to do this.) |  |
| Knock icicles off eaves. |  |
| Clear snow from outdoor dryer vent and other exhausts. |  |
| Check water main/meter or well pump for leaks or sweating. |  |
|  |  |
| **Fall Winter Inside** |  |
| Check date of Fire Extinguisher. |  |
| Check for signs of water leaks/damage. |  |
| Check operation of windows and doors. Repair as needed. |  |
| Remove shower head and sink aerators and soak in vinegar to dissolve hard water deposits. |  |
| Check smoke and CO alarms. Change batteries when you set your clocks back at the end of Daylight Savings. |  |

****

**HOME MAINTENANCE CHECKLIST: FALL - WINTER**